Date: May 17, 2016

Name: Haofu Zhu

I did some research on magnetometer calibrating and successfully calibrate the IMU according the local magnetic field which is hard-iron calibration. The stepper can move based on the IMU’s reading now and the movement is quite stable. I will assist Jinlun with the calibrated IMU tomorrow.