Date: May 26, 2016

Name: Haofu Zhu

After some research, I found that the transceiver itself has a checking method that avoid interfere from other machine when they are using the same frequency. It can be done by changing their address of package header. The transceiver will not react to the message with different address. So it is possible that we can avoid interfere. The new problem is that how we can let both the transmitter and receiver determine the address automatically. I am still working on it.